A black background with blue text

Description automatically generated with low confidence

**Materia**[:](https://m.itculiacan.edu.mx/course/view.php?id=395)

Conmutación y Enrutamiento de Redes

**Tarea**:

Evidencia script de configuración

**Alumno**:

José Alberto Angulo López

**Maestro**:

Angelica Ramírez Salazar

**Carrera**:

Ingeniería en Sistemas Computacionales

A diagram of a triangle

Description automatically generated

*!================R1===================!*

enable

configure terminal

hostname R1

no ip domain-lookup

no logging console

interface LOOPBACK1

  ip address 170.17.0.1 255.255.255.0

no shutdown

interface Serial0/0/0

  ip address 10.0.0.1 255.255.255.252

no shutdown

interface Serial0/0/1

  ip address 10.0.0.10 255.255.255.252

no shutdown

*!Enrutamiento*

*!R2*

ip route 172.16.0.0 255.255.0.0 10.0.0.2

*!R3*

ip route 200.33.18.0 255.255.255.0 10.0.0.2

*!================R2===================!*

enable

configure terminal

hostname R2

no ip domain-lookup

no logging console

interface GigabitEthernet0/0

*description Lan R2*

  ip address 172.16.0.1 255.255.0.0

no shutdown

interface Serial0/0/0

  ip address 10.0.0.5 255.255.255.252

no shutdown

interface Serial0/0/1

  ip address 10.0.0.2 255.255.255.252

no shutdown

*!Enrutamiento*

*!R1*

ip route 170.17.0.0 255.255.255.0 10.0.0.6

*!R3*

ip route 200.33.18.0 255.255.255.0 10.0.0.6

*!================Sw2===================!*

enable

configure terminal

hostname Sw2

no ip domain-lookup

no logging console

interface vlan 1

*description Lan Switch*

  ip address 172.16.0.2 255.255.0.0

no shutdown

*!================R3===================!*

enable

configure terminal

hostname R3

no ip domain-lookup

no logging console

interface GigabitEthernet0/0

*description Lan R2*

  ip address 200.33.18.1 255.255.255.0

no shutdown

interface Serial0/0/0

  ip address 10.0.0.9 255.255.255.252

no shutdown

interface Serial0/0/1

  ip address 10.0.0.6 255.255.255.252

no shutdown

*!Enrutamiento*

*!R1*

ip route 170.17.0.0 255.255.255.0 10.0.0.10

*!R2*

ip route 172.16.0.0 255.255.0.0 10.0.0.10

*!================Sw3===================!*

enable

configure terminal

hostname Sw3

no ip domain-lookup

no logging console

interface vlan 1

*description Lan Switch*

  ip address 200.33.18.2 255.255.255.0

no shutdown